|  |  |  |
| --- | --- | --- |
|  |  | |
|  |  |  |
| **Mika**  **Pendant Range**  LED Pendants |  | Data Sheet |
|  |

|  |  |  |
| --- | --- | --- |
| **Product Information**  The Mika range of pendant luminaires are perfect for counter/table lighting in commercial or domestic applications. With a range of colour options and wattages.  They come complete with a 2 year warranty for your peace of mind. |  | **Product Features**   * 2 year warranty * High efficiency * IP20 * 9W or 24W 3000K LED * CRI: Ra82 * Non-Dimmable * 55° Beam angle * 5 Colour options * Fully integrated driver * Lighting designers can download photometric data from our website * L70 - 30,000 hours |

**Product Specification**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Product Code** | **Product Description** | **Wattage (W)** | **CCT (K)** | **Lumens (lm)** | **CRI (Ra)** | **Energy Efficiency Class** | **Protection Class** |
| KSR7270 | Mika 9W 3000K LED Pendant Light White with White Shade | 9 | 3000 | 780 | 82 | A+ | I |
| KSR7271 | Mika 9W 3000K LED Pendant Light White with Transparent Shade | 9 | 3000 | 780 | 82 | A+ | I |
| KSR7272 | Mika 9W 3000K LED Pendant Light Black with Smoke Transparent Shade | 9 | 3000 | 780 | 82 | A+ | I |
| KSR7273 | Mika 9W 3000K LED Pendant Light Black with Black/Gold Shade | 9 | 3000 | 780 | 82 | A+ | I |
| KSR7274 | Mika 9W 3000K LED Pendant Light Aluminium with Transparent Shade | 9 | 3000 | 780 | 82 | A+ | I |
| KSR7275 | Mika 24W 3000K LED Pendant Light White with White Shade | 9 | 3000 | 2150 | 82 | A+ | I |
| KSR7276 | Mika 24W 3000K LED Pendant Light White with Transparent Shade | 9 | 3000 | 2150 | 82 | A+ | I |
| KSR7277 | Mika 24W 3000K LED Pendant Light Black with Smoke Transparent Shade | 9 | 3000 | 2150 | 82 | A+ | I |
| KSR7278 | Mika 24W 3000K LED Pendant Light Black with Black/Gold Shade | 9 | 3000 | 2150 | 82 | A+ | I |
| KSR7279 | Mika 24W 3000K LED Pendant Light Aluminium with Transparent Shade | 9 | 3000 | 2150 | 82 | A+ | I |
| KSR7306 | Mika Nu 9W 3000K LED Pendant Light Black | 9 | 3000 | 780 | 82 | A+ | I |
| KSR7307 | Mika Nu 9W 3000K LED Pendant Light White | 9 | 3000 | 780 | 82 | A+ | I |
| KSR7308 | Mika Nu 9W 3000K LED Pendant Light Aluminium | 9 | 3000 | 780 | 82 | A+ | I |
| KSR7309 | Mika Nu 24W 3000K LED Pendant Light Black | 9 | 3000 | 2150 | 82 | A+ | I |
| KSR7310 | Mika Nu 24W 3000K LED Pendant Light White | 9 | 3000 | 2150 | 82 | A+ | I |
| KSR7311 | Mika Nu 24W 3000K LED Pendant Light Aluminium | 9 | 3000 | 2150 | 82 | A+ | I |

|  |  |
| --- | --- |
| **Nominal voltage** | 220~240V |
| **Operating frequency** | 50-60Hz |
| **Ambient temperature range** | -20°c~+40°c |
| **Start time** | < 0.5 sec |
| **Beam angle** | 55° |
| **IP rating** | 20 |

**Construction**

|  |  |
| --- | --- |
| Body: | Aluminium |
| Diffuser: | Polycarbonate |

**Standards**

|  |  |
| --- | --- |
| BSEN60598-1:2015 | Luminaires – Part 1: General requirements and tests |

**In Conformity with**

|  |  |
| --- | --- |
| LVD | Low voltage directive 2014/35/EU |
| EMC | Electromagnetic compatibility directive 2014/30/EU |
| ERP | Energy related products directive 2009/125/EC |
| RoHS | Restriction of hazardous substances 2011/65/EU |

**Product Dimensions**

|  |  |  |
| --- | --- | --- |
|  |  |  |
| **KSR7270-7274** | **KSR7275-7279** | **KSR7306-7308** |
|  |  |  |
| **KSR7309-7311** |  |  |

KSR Lighting is constantly developing and improving its products. For this reason, all product descriptions in this data sheet are intended as a general guide, and KSR may change specifications from time to time in the interest of product development, without prior notification or public announcement. All descriptions in this data sheet present only general particulars of the goods to which they refer and shall not form part of any contract. Data in this guide has been obtained in controlled experimental conditions. However, KSR Lighting cannot accept any liability arising from the reliance on such data to the extent permitted.